GenLib User's Manual
<<< Previous |  |

# DPGEN_SFFT

## Name

DPGEN_SFFT -- Static Flip-Flop with Scan-Path Macro-Generator

## Synopsis

    #include  <genlib.h>

``void `GENLIB_MACRO``(DPGEN_SFFT, char *`modelname`, long `flags`, long `N`);`

## Description

Generate a N bits static flip-flop with scan-path named modelname. The two latches of this flip-flop are i.e. each one is made of two interters looped togethers.

How it works :

- `scan` when set to `'1'` enables the scan-path mode. Note that in scan-path mode, the `wen` signal is not effective.

- `scin` : the input of the scan-path. This terminal is different from `i0[0]`.

  The `scout` is `q[N-1]` (in the following example this is `q[31]`).

- `wen` when set to `'1'` enables the writing of the flip-flop.

### Terminal Names

1. `scan` : scan-path mode (input, 1 bit).

2. `scin` : scan path in (input, 1 bit).

3. `wen` : write enable (input, 1 bit).

4. `ck` : clock signal (input, 1 bit).

5. `i0` : data input (N bits).

6. `q` : output (N bits).

7. `vdd` : power.

8. `vss` : ground.

## Example

    GENLIB_MACRO(DPGEN_SFFT, "model_sfft_32"
                           , F_BEHAV|F_PLACE
                           , 32
                           );

    GENLIB_LOINS( "model_sfft_32"
                , "instance1_sfft_32"
                , "scan"
                , "scin"
                , "wen"
                , "ck"
                , "i0[31:0]"
                ,  "q[31:0]"  /* a[31] is "scout". */
                , "vdd", "vss", NULL
                );

## See Also

GENLIB_MACRO(3), genlib(1)

<<< Previous | Home |
DPGEN_SFF | Up |