GenLib User's Manual
<<< Previous |  | Next >>>

# DPGEN_AND4

## Name

DPGEN_AND4 -- AND4 Macro-Generator

## Synopsis

    #include  <genlib.h>

``void `GENLIB_MACRO``(DPGEN_AND4, char *`modelname`, long `flags`, long `N`, long `drive`);`

## Description

Generate a N bits four inputs AND with an output power of drive named modelname.

Valid drive are : 2 or 4.

### Terminal Names

1. `i3` : input.

2. `i2` : input.

3. `i1` : input.

4. `i0` : input.

5. `q` : output.

6. `vdd` : power.

7. `vss` : ground.

### Behavior

q <= i0 and i1 and i2 and i3

## Example

    GENLIB_MACRO(DPGEN_AND4, "model_and4_32"
                            , F_BEHAV|F_PLACE
                            , 32
                            , 2
                            );

    GENLIB_LOINS( "model_and4_32"
                , "instance1_and4_32"
                , "i3[31:0]"
                , "i2[31:0]"
                , "i1[31:0]"
                , "i0[31:0]"
                ,  "q[31:0]"
                , "vdd", "vss", NULL
                );

## See Also

GENLIB_MACRO(3), genlib(1)

<<< Previous | Home | Next >>>
DPGEN_AND3 | Up | DPGEN_NOR2