#      Copyright (c) 1997 by Cadence. All rights reserved.      
###################################################################
# In each of TOP()/BOTTOM()/LEFT()/RIGHT() section, there are     #
# placed IOs. In the IGNORE() section, the IOs are ignored        #
# by the IOPlacer. In every section, the IO syntax could be:      #
#        for pin:       (IOPIN iopinName.0 );                       #
#        for pad:       iopadName orientation ;                   #
#        for space:     SPACE  value;                             #
# The capital words are keywords. orientation is not required.    #
# The value is the space between the IO above and the IO below it.#
###################################################################

TOP ( # IOs are ordered from left to right
   (IOPIN b(3).0 );
   (IOPIN cin.0 );
   (IOPIN ck.0 );
   (IOPIN cout.0 );
   (IOPIN d(0).0 );
   (IOPIN d(1).0 );
   (IOPIN d(2).0 );
   (IOPIN d(3).0 );
   (IOPIN fonc.0 );
   (IOPIN i(0).0 );
   (IOPIN i(1).0 );
   (IOPIN i(2).0 );
   (IOPIN a(0).0 );
   (IOPIN a(1).0 );
   (IOPIN a(2).0 );
   (IOPIN a(3).0 );
   (IOPIN ng.0 );
   (IOPIN acc_i_down.0 );
   (IOPIN acc_i_up.0 );
   (IOPIN acc_o_down.0 );
   (IOPIN acc_o_up.0 );
   (IOPIN b(0).0 );
   (IOPIN b(1).0 );
   (IOPIN b(2).0 );

)
BOTTOM ( # IOs are ordered from left to right
   (IOPIN i(3).0 );
   (IOPIN i(4).0 );
   (IOPIN i(5).0 );
   (IOPIN i(6).0 );
   (IOPIN i(7).0 );
   (IOPIN i(8).0 );
   (IOPIN noe.0 );
   (IOPIN np.0 );
   (IOPIN oe.0 );
   (IOPIN over.0 );
   (IOPIN ram_i_down.0 );
   (IOPIN ram_i_up.0 );
   (IOPIN ram_o_down.0 );
   (IOPIN ram_o_up.0 );
   (IOPIN scin.0 );
   (IOPIN sh_left.0 );
   (IOPIN sh_right.0 );
   (IOPIN test.0 );
   (IOPIN y(0).0 );
   (IOPIN y(1).0 );
   (IOPIN y(2).0 );
   (IOPIN y(3).0 );
   (IOPIN zero.0 );
)
IGNORE ( # IOs are ignored(not placed) by IO Placer
)
